

ADDENDUM #1

RFQ 24-005

**Saddlecreek Ct. Tack Coat**

This addendum is being issued to address questions submitted on RFQ 24-005.

The following needs to be changed. The specifications are incorrect and need to be changed as follows:

1-The proposal needs to state that 1 ½” of existing asphalt needs to be milled out.

2-Pave ½” with OGI.

3-Overlay with 1 ½” of 9.5 MM surface coarse.

4-paint center line.

This addendum should be signed and returned with your proposal.

Sunshine Palmer

Purchaser

City of Auburn, Georgia

Company Name

Authorized Representative

Page **1** of **1**